IP Multicasting over ATM: The Multicube

Approach

H. Schulzrinne, M. Smirnov, R. Roth, A. Wolisz

GMD FOKUS, Hardenbergplatz 2, Berlin 10623, Germany

Tel.: +49 30 25499200 Fax.: +49 30 25499202

Abstract. This paper gives practical information along with theoretical background

on Multicube project design decisions for scalable and reliable multicast service

facilitating multimedia interworking of real users over the European ATM pilot. IP

multicast mapping is proposed to be performed with the use of a minimal address

resolution server serving a special multicast LIS within the ATM LAN. The

feasibility of this choice is proved partly by practical experiment partly via

simulation. Data applications for CSCW scenarios depend on a reliable information

transfer. The Multicube project selected Xy, an X application sharing tool, to study

the reliable multicast services provided by the protocols MTP, RMP and SRM.

1. Introduction

How should applications use the multipoint functionality offered by ATM? Interoperability

across internetworks and the use of existing applications suggests the use of IP multicast

over ATM. This, however, requires additional mappings and address resolutions. The paper

discusses alternatives and reasons behind the current decision for the Multicube project [1].

The objective of Multicube is to develop, test and validate an ATM-based multipoint

infrastructure for the support of CSCW applications. It is a trial-oriented project with the

participation of end users from the automotive and aerospace industry. The majority of their

multicast applications are IP based.

IP multicast is maturing fast. It currently supports teleconferencing, teleteaching, virtual

meetings. It is involving more complex CSCW applications spread around the globe, like

distributed simulation and collaborative CAD. The underlying internetwork tends to

migrate towards gigabit technologies deploying ATM local and wide area networks. At

present, however, ATM connectivity is concentrated mainly within user premises.

Consequently, these islands are treated as Logical IP Subnetworks (LIS). One of the main

differences with regard to multicasting is in different addressing schemes in LANs with

native broadcast capabilities and ATM networks without this service. The addressing

mechanisms in the Internet and, generally, in IP subnets make use of common flat

availability of any pair of stations within the IP subnet address space (all hubs, bridges,

switches, etc. are invisible). This feature causes no serious problems for address resolution tasks within legacy IP subnets such as Ethernet. Address Resolution Protocol (ARP) queries

are broadcast, an operation which is cheap and natural for these networks. On the contrary,

in the ATM environment, switches play a more visible role. ATM service model is

connection oriented, broadcast is not a natural operation and, therefore, address resolution

grows to become one of the major problems for IP multicast over ATM. Hence, ATM is an

example of the so called NBMA (Non-Broadcast Multiple Access). IP multicast uses a

special multicast address, derived from a reserved Class D Internet address space. A host

sends its multicast flow to this address and subscribes itself to this address at the nearest

multicast router to receive the flow. Operation of joining the multicast group is receiver

initiated. NBMA multicast is to be organised via explicit connection establishment from

sender(s) to receivers. A special kind of point-to-multipoint connection is specified within

the UNI 3.1 signalling for multicast. However, joining the multicast group in NBMA is

possible only via the root of the point-to-multipoint connection, i.e. the root has to know all

NSAP addresses for all receivers.

The Multicube design approach tries to offer a seamless internetworking across private

and public domains in a heterogeneous environment. Its strategy allows a smooth migration

of existing applications and prevents application development to be locked onto a particular

technology. Current understanding of the main project challenge is to achieve several levels

of interoperability: between automotive and aerospace users and network designers,

between different applications (across hardware and software), between IP and ATM styles

of addressing, resource reservation, session management, multicasting, and, finally,

between signalling stacks of private and public ATM networks.

The paper concentrates on design alternatives and their evaluation aiming at making

general feasibility recommendations in the following areas.

1. Reliable multicast for X application sharing . IP multicasting offers only an unreliable

datagram delivery. Transport protocols add the reliability needed by application sharing.

TCP provides reliability in the case of unicast communication, but cannot be extended for

group communication. Multicube is exploring alternative proposals for reliable multicast

transport protocols, comparing them with respect to performance and scalability. As the

required reliability services depend much on the particular application, Multicube has

chosen to concentrate on X application sharing in its experiments. This section of the paper

gives an overview of the methods selected in the project and experiments planned.

2. Mapping of IP multicast to ATM point-to-multipoint connections . This effort is

intended to propose and validate efficient mechanism for IP multicast applications over

ATM LANs interconnected via public ATM network. We propose a minimal (as compared

to G. Armitage’s MARS [2]) multicast address resolution server (mARS). mARS supports

multipoint-to-multipoint connections and leaf initiated join for UNI 3.1 and 4.0. Its

extension supports different QoS levels for the same multicast group. Today´s architectural

alternatives are examined with the use of simulation for different scenarios of address

resolution and multicast in ATM LANs.

3. Implementation issues . Several alternatives for the implementation of IP multicast

over ATM were examined including FORE SPANS signalling (with broadcast ARP),

FORE UNI 3.0 signalling (with Classical IP over ATM ARP), Vendor Independent

Network Control Entity (VINCE) by ARPA and NRL, and MARS using Q.port (Portable

ATM Signalling Software) by Bellcore. Comparison of existing alternatives is made in

terms of feasibility, practical availability of software components, their conformance to

existing ITU-T and ATM Forum standards, interoperability and generality.

2. Reliable multicast for X application sharing

Besides audio/video services that can be run over an unreliable IP multicasting service,

there are other CSCW applications depending on a reliable information transfer. So issues

of reliable multicast become relevant to the Multicube project. The main focus for reliable

multicast will lie on questions of scalability. Different solutions will be compared for

efficiency in handling larger user groups distributed over a wide area network. Since

reliability requirements depend much on the particular application under consideration,

Multicube will concentrate on an appropriate application and study the behaviour of several

reliable multicast protocols in their capabilities of providing support.

The Multicube demonstration example is an X application sharing tool that will allow to

contrast TCP based unicast with the multicast service provided by the protocols MTP, RMP

and SRM. The experiments will include mixed traffic scenarios with parallel real-time

audio / video transmission, allowing to study integration with resource reservation.

2.1 X Application Sharing for Multicube

With X application sharing tools, single-user X Window applications can readily be

introduced into group conferences. Under the X window system a client application can be

run on a different system than the X server which controls display and input devices.

Communication between X client and X server is achieved by message exchange using the

X protocol. An X application sharing tool intercepts these messages and re-distributes them

among several users.

The original X Window system, however, has not been designed for a group

environment, hence the development of an application sharing tool becomes non-trivial ([3,

4]). The main difficulty arises from the fact that X messages may contain atoms , which are

unique identifiers private to the X server. This prevents the simple replication of client

requests to all servers, instead they need a translation to local settings. Dynamic conference

behaviour like late joining or temporarily leaving participants is hard to accommodate in X,

as the exact knowledge on current resources such as windows, pop-up menus, dialogue

boxes, together with their actual attribute values is kept at the X server and is not available

at the client-side. Simple strategies that archive all preceding messages for replay at the

late-comer become prohibitive, because it would make join latency for the new participant a

function of the previous duration of the conference.

2.2 Xy - an X Application Sharing Tool

Multicube selected for its experiments the X application sharing tool Xy [5]. The basic idea

for Xy is to use an displayless X server as part of the distributed sharing component. This

Xy server does not control I/O devices directly, but interacts with Xy agents local to the

participant (see Figure 1).

Xy can fulfil the requirements on scalable X application sharing. It is fully transparent to

X Clients and X servers: a client notices no difference when communicating with the Xy

server to any other ordinary single-user X server. But also the X servers at the participant

side need no modification, as the local Xy agent will emulate to them X client behaviour in

a consistent way.The distribution of the sharing component opens up the possibility for

exploiting multicast communication capabilities. An identical request message from an X

client can be multicast via the X server to all Xy agents, and there the message is translated

for the local X server. The local Xy agent also handles heterogeneity in system capabilities

like pixel resolution, colour model, substitution of locally unavailable font families etc.

unicast

multicast

Efficiency is guaranteed, since those requests that can already be responded by the Xy

server need not be distributed over the network; and not all events need to be reported back;

but some are already filtered out locally by the Xy agent. For instance only cursor

movement from the current input token holder are transmitted, while corresponding events

at other displays are discarded.

Accommodation of late-comers causes no problem to Xy, since all required information

to instantiate the X server of a new participant is accessible in the Xy server. Xy even

allows to close a conference temporarily and to resume it at a later stage in exactly the same

state as before with no need for terminating running applications. This feature gives

mobility to participants who can close a session on one machine and resume it on another.

2.3 Reliable Multicast Protocols

A large collection of proposals for reliable multicast protocols has been developed in recent

years [6]. The service that they provide differs in adopted acknowledgement strategy, order

preserving capabilities, supported atomicity and flow control.

Coordination between senders and receivers can be done explicitly by positive

acknowledgement as it is done e.g. in TCP for the unicast case. Positive ACKs by all

receivers for each packet sent, however, may easily become inefficient if not impossible for

large groups. So trade-offs are needed to secure scalability with growth in group size.

Negative acknowledgements are often better suited. Correct delivery is assumed and only

lost or corrupted packets are reported back to the sender for retransmission.

In a multicast transmission, there can be several concurrent senders to a group, hence we

can distinguish different degrees of sequence preservation for the receivers. Under source

ordering, the packets are only ordered in sequence for each sending source, and these

streams may be interleaved arbitrarily at each receiver; under total ordering, in contrast,

each receiver gets all messages in exactly the same sequence. For the maintenance of a

consistent state at all receivers, some applications require atomicity of packet transmission;

i.e. a message is either received by all group members or by none at all.

Flow control prevents the sender from sending at a bandwidth higher than receivers can

handle. Mechanisms for flow control may set the length of the sender window buffer, or be

rate controlled, changing the frequency by which a sender can send out packets. The latter

policy is especially appropriate for protocols using negative acknowledgements. For its

X

Client

1

X

Client

m

Xy

Server

Xy

Agent

1

Xy

Agent

2

X

Agent

n

X

Server

1

X

Server

2

X

Server

n

··· ···

··· multiplexing translation /

filtering

Xy Control

register, add

remove, close

share, input, ...

Fig. 1 Xy Architecture experiments, Multicube has chosen three protocols that will be compared for supporting X

application sharing sessions: MTP, RMP and SRM.

2.3.1 MTP - Multicast Transport Protocol

The Multicast Transport Protocol was defined in RFC 1301 [7]. It describes a protocol for

reliable transport that utilizes the multicast capability of lower layer networking

architectures. MTP is based on a token scheme and can provide atomicity and total ordering

service. A group under MTP is known as a web . One member of the web is designated as

master that controls the communication. It hands out send-tokens to producers , for sending

data packets to the consumers in the web.

Transmission in MTP is rate based, the heartbeat is a time interval, during which only a

fixed number of packets may be sent by a producer holding the send token. The retention

value sets the number of heartbeats how long a sender must keep a packet buffered for

possible retransmission. During that time, consumers can send NACKs in case they detect

lost packets. The master sends out message acceptance records by which atomicity of

packet reception in the group is controlled.

The variant of MTP that will be used in Multicube is the protocol named MTP-2 [8],

which offers improvements in functionality and efficiency. MTP-2 adds recovery

procedures for master failures and migration of the master side. Beside total ordering MTP-

2 can also support weaker notions of message order. MTP-2 has been implemented in user

mode and as a kernel driver for SunOS 5.

2.3.2 RMP - Reliable Multicast Protocol

Reliable Multicast Protocol (RMP) [9] provides a reliable multicast service on top of the

unreliable multicast datagram of IP multicasting. It is based on a token ring technique and

uses a combination of positive and negative acknowledgements (ACKs/NACKs) for error

detection and delivery confirmation. With RMP the user can choose between different

reliability guarantees which are selectable on a per packet basis. The QoS level ranges from

unreliable, reliable, source ordered, totally ordered, and various levels of atomicity. The

selected QoS level determines the ACK or NACK policy; an increase in the level of QoS

has to be paid off with latency of packet delivery.

In RMP a token rotates in the group. The token holder is responsible to send out a

positive ACK which contains information on the order and timestamps of received data

packets so far, and then passes the token on. Based on the ACK message, members can

detect lost packets and request retransmission by NACKs. A member only accepts the

token, until it has received all previous messages. Thus, complete delivery of a packet can

be detected after full rotation of the token.

RMP allows dynamic joining and leaving of group members. With special request

packets, membership changes are signalled to the group members. RMP offers flow and

congestion control based on a modified sliding window protocol similar to the algorithms

used in TCP.

2.3.3 SRM (Scalable Reliable Multicast)

SRM (Scalable Reliable Multicast) [10] is not a fixed protocol but more of a framework in

which reliable multicast services can be realized. The design of SRM is based on the idea of

application level framing (ALF) and light-weight sessions. Under ALF functionality and

flexibility is left to the application as much as possible.

Consequently, SRM assumes only a minimal delivery model for reliability, interpreted

as eventual delivery of all data to all group members without enforcing any particular

delivery order; the responsibility for stricter requirements is transferred to the particular

application.

The SRM group model is closely modelled to the anonymous host group model of IP

multicast allowing multiple senders and dynamic join/leave operations. Efficiency and

scalability to very large groups is achieved by extending error recovery actions to all group

members. Not only the sender alone, but any member that has correctly received a data

packet can answer the retransmission request from a group member. By dynamically

adjusting latency and response delay parameters, implosion of identical retransmission

requests and repair packets is avoided, and thus a self-organising distributed error recovery

system is installed.

The SRM framework has been prototyped in , a distributed whiteboard application,

and has been extensively tested on a global scale with sessions ranging from a few to more

than 1000 participants.

Given the characteristics of SRM, it qualifies as one of the prime candidates to be

applied in Multicube. The adaptation of the SRM framework to X application sharing will

be an important outcome of the experiments on X application sharing in Multicube.

3. Mapping of IP multicast to ATM point-to-multipoint connections

3.1 A Minimal Address Resolution Server

Convergence of IP and ATM service models [11] will require a full `IP service´ over ATM:

multicast group management (IGMP [12, 13]), multicast flow distribution with receiver

initiated joins, leaves, and QoS specifications. This convergence is supported by about 30

relevant IETF RFCs and drafts centered around Classical IP over ATM [14], vendor

implementations, the MPOA work within the ATM Forum [15] and new features in UNI

4.0 draft following the IP service model. Table 1 gives an overview of the IP multicasting

over ATM problem area.

A Minimal Address Resolution Server (mARS) was proposed in [16] for the

MULTICUBE consortium partners to enable IP multicast experimentation over the

European ATM pilot. Interconnection of the partners´ ATM islands could be achieved with

the use of PVCs or with a specially designed type of call facilitating multipoint-to-

multipoint connections in a public ATM network. Major mARS features are as follows:

¯ mARS is intended to resolve only IP Class D (multicast) addresses to NSAP addresses

(in contrast to G. Armitage´s MARS that resolves both unicast and multicast addresses).

¯ mARS is to be used within the so-called multicast Logical IP Subnet (mLIS) while the

regular unicast ARP is to be performed within Classical IP over ATM; like the IP

Table 1:

IP ATM

Connectionless X Connection-oriented

Only a single host needs to reply to Áll hosts´´query Every host is to be queried directly and has to

answer individually, endpoints registration is

required

Receiver initiated join for the established MCT Root initiated join only [UNI 3.1]

Total availability and knowledge of IP addressing Need for ARP and ARP server

Various algorithms for the MCT construction Use of multicast servers and/or meshes of VCs

Special means for QoS assurance (RSVP, etc.) QoS assurance is a part of signalling multicast which uses a separate address space within a connectionless environment, the

mARS proposal suggests to separate LISs within a connection-oriented environment,

where the above structuring of the address space is impossible.

¯ To avoid confusion with the existing Classical IP over ATM ARP server, mLIS could be

configured as a private IP subnet within the MULTICUBE partner´ premises; a single

mLIS can serve a number of Classical LISs co-existing in a given ATM environment.

¯ The mARS implementation is to be based on the FORE atmarp source, extended to

enable multiple NSAP addresses to be mapped to a single (Class D) IP address.

¯ mARS operation will be most beneficial for ATM networks with UNI 3.1/UNI 4.0

signalling, but also can be used together with the FORE IP.

Two issues should be distinguished: a/. How is the address resolution for IP multicast

over ATM done? and b/. How actually the multicast flow is distributed? Table 2 shows

these issues (with interfaces used - Int ) for three schemes examined via simulation (section

3.2). Practically, nowadays the mARS scenario implies that each workstation, equipped

with the ATM driver, should be configured to have qaa0 interface for Classical IP, fa0 - for

FORE IP, and, say, qaa2 - for mLIS. The qaa0 and qaa2 should know NSAP addresses for

Classical IP over ATM ARP and mARS respectively. The fa0 will use the FORE IP ARP.

Table 2 shows two motivations for mARS: it decreases the SCP load by avoiding broadcast

ARP and saves the bandwidth via utilisation of hardware cells duplication. Thus a

workstation subscribes itself to a particular multicast group with mARS via qaa2 interface

and then receives the multicast flow via fa0 (or any of qaXX, faX when UNI 3.1/UNI 4.0

will become available). This is possible because the ForeRunner SBA-200 ATM SBus

adapter inside the workstation serves also as a router between different connected LISs.

3.2 Simulation results

The above schemes were simulated within the discrete event domain of the Ptolemy

modelling tool [17]. All experiments assume that a local ATM network has a FORE ATM

switch (say, the ForeRunner ASX-200) supporting the above mentioned assumptions and

that the SCP´s processing capacity ( C ) is shared among the following types of load: unicast

connection establishment and maintenance, multicast connections establishment and

maintenance, connectionless service (with lower priority). According to [18] C = 100

calls/s. The load is produced by FORE IP for a broadcast ARP. Independent parameters for

each run of the simulation are: Unicast Call Load ( UCL ) and Multicast Call Load ( MCL ).

Address Resolution Load in terms of Connectionless Load (for FORE IP ARP) or Classical

ARP Load (for Classical IP over ATM) is defined by UCL and MCL . Independent

parameters are measured in terms of percentage of C . Obviously, at any time UCL + MCL

should not exceed the total C .

Basically, two different cases should be considered: Classical IP ARP implemented at

switch and Classical IP ARP implemented at other location (endpoint, router). In the latter

case the SCP has the increase of its unicast load due to the necessity to establish on demand

Name óf

scheme

Address Resolution Multicast

How Int. How Int.

CLS By Connectionless Server (CLS) in

Switch Control Processor (SCP) fa0 Cells duplication by switch hardware;

point-to-multipoint connections fa0

ClIP By Classical IP over ATM ARP qaa0 Cells duplication in host, mesh of point-

to-point connections qaa0

mARS By mARS in mLIS qaa2 Cells duplication by switch´ hardware;

point-to-multipoint connection fa0

Table 2:

and maintain PVCs from endpoints to the ARP server. When the Classical IP ARP server

implementation occurs within the switch it also decreases the switch productivity. This

paper neglects the difference between these two cases. We also assume that all endpoints

are directly connected to the switch, that Classical IP over ATM follows the RFC 1577 and

its timing defaults (for endpoint´s ARP cache ageing for example).

Simulation results are summarised in Tables 3 to 6. Each simulation ran for 1000

simulated seconds which corresponds to simulation of 10000 to 80000 calls established for

each of the considered variants. In all of these experiments the switching fabric

performance was not considered - only SCP performance was taken into account in terms of

minimal connection establishment delay ( SCPmin = 1/C ). The major output of the model

was called a Multicast Connection Latency which consists of ARP delay and connection

establishment delay ( CEdelay ). CEdelay is a function of SCPmin (1 + UCL + MCL) .

Actual instance of CEdelay (to model connection establishment to a host or to an ARP

server) was considered randomly chosen out of the interval [ 0.8·CEdelay, 3.6·CEdelay ].

These coefficients were measured in the GMD FOKUS IP over ATM environment; details

on simulation tuning and organisation could be found in [20].

According to [18] the CLS service is considered to have a lower priority for an SCP in

comparison with connections establishment. This situation is reflected in the model as well

as hardware multicast ( CLS ), mesh of point-to-multipoint connections ( ClIP ), and mLIS

usage only for multicast ARP queries ( mARS ).

Table 3:

Multicast connection latency [sec] as a function of unicast call load (UCL)

UCL = 0.1 0.2 0.4 0.6 0.8

mARS 0.104 0.099 0.168 0.264 0.380

ClIP 0.262 0.287 0.329 0.377 0.415

CLS 0.886 1.298 2.630 3.365 5.90

Table 4:

Multicast connection latency [sec] as a function of multicast call load (MCL)

MCL = 0.1 0.2 0.4 0.6 0.8

mARS 0.104 0.050 0.044 0.052 0.059

ClIP 0.262 0.291 0.328 0.372 0.415

CLS 0.886 0.708 0.697 0.708 0.739

Table 5:

Multicast connection latency [sec] as a function of a group size (M)

M = 1 5 8 10 11 16

mARS 0.066 0.067 0.067 0.067 0.066 0.066

ClIP 0.066 0.164 0.268 0.328 0.361 0.521

CLS 0.993 1.062 1.062 1.096 1.034 1.112

Table 6:

Multicast connection latency [sec] as a function of # of active ports (P) in a switch

P = 10 12 16 24

mARS 0.066 0.066 0.067 0.066

ClIP 0.325 0.329 0.325 0.329

CLS 0.661 0.798 1.049 1.635

Tables 1 and 2 assume that the load which is not varying in the experiment is UCL/MCL = 0.1 (i.e. 10%

of the maximal switch load C); the number of multicast group members M = 10; the number of active switch

ports P = 16. For Tables 3 and 4 UCL = MCL = 0.25 (25% of C each, which constitutes 50% of C in total).

Some results:

1. CLS case has the largest latency (due to a broadcast implementation and, mainly, due

to a lower priority); it depends linearly on the number of active ports (P); and non-linearly

on the unicast load. The CLS case is generally less effective than ClIP or mARS but, nevertheless, it scales well in terms of MCL growth and the group size growth. The CLS is

the only scheme where ARP and Call Establishment are not separated.

2. ClIP case with a mesh of point-to-point connections has the 2nd largest latency

(however, 2 - 10 times less than that of CLS) which depends linearly on the number of

receivers (each newcomer to the group requires both the ARP service and a separate point-

to-point connection); it´s the only scheme which depends on the MCL growth.

3. Minimal address resolution server shows the smallest latency and scales well in terms

of all parameters: UCL, MCL, M, and P. This is due to combination of a separate mLIS and

the hardware multicast.

4. Implementation Issues

The following implementation alternatives were considered within the project: FORE

SPANS signalling, FORE UNI 3.0 signalling, Vendor Independent Network Control Entity

(VINCE) by ARPA and NRL, and Q.port (Portable ATM Signalling Software) by Bellcore.

It´s important to mention here that the multicast capable MARS [2] by G. Armitage is

available as public domain software in a source code except the Q.port. Almost all of the

project participants are using FORE equipment on their premises, therefore dependence on

a different signalling was considered as a disadvantage. VINCE, available as public domain

software in a source code, was considered as an alternative, especially for the reason of its

vendor independence. However, the lack of experience with VINCE and its non-standard

NSAP format has turned the project´ choice in favour of decisions supported by FORE -

UNI 3.0 signalling and SPANS signalling. Availability of FORE source code for needed

utilities was also a factor.

Unfortunately, it turned out that current release of ForeThought 3.0.2 software does not

support the add_party primitive which is needed for a point-to-multipoint call. It will be

supported with other UNI 3.1 features only in a next release. In parallel to waiting for this

new release it was decided to start implementation of mARS.

So far, each ATM LAN will be configured to have at least two logically separated LISs -

one for Classical IP over ATM with unicast address resolution, and another with multicast

address resolution. To avoid a full mesh of point-to-point connections over ClIP it is

recommended to use FORE IP with hardware multicast capability. ARP overhead shown by

simulation is considered less harmful than completely inefficient bandwidth utilisation in

case of mesh. This solution was implemented within the networking infrastructure of GMD

FOKUS and demonstrated with the use of integrated multimedia conferencing tool isc

[19].

The lessons learned so far on implementation are as follows:

¯ Multicast applications can run successfully within the FORE IP logical subnetworks in

parallel with the ClIP LIS, co-existing for the same physical structure.

¯ FORE ATM adapter software serves as a router (inside multihomed hosts) between

different LISs (including Ethernet, several Classical and FORE IP LISs).

¯ FORE IP uses hardware cells duplication which makes it effective for the distribution of

the multicast flow but not for the broadcast ARP, because the CLS becomes a bottleneck

in case of high call load.

¯ based on simulation results, due to the separation of LISs, the mARS altern ative could

be considered as the best available choice in terms of efficiency, scalability, and

implementation efforts.

References

1. MULTICUBE - Efficient MULTIpoint to MULTIpoint broadband switched network

services for distributed MULTImedia applications , ACTS project AC012, home page at

http://www.cselt.stet.it/sonah/MULTICUBE/index.html

2. Armitage, G. Support for Multicast over UNI 3.0/3.1 based ATM Networks, Internet draft

<draft-ietf-ipatm-ipmc-12>, February, 1996, 83 pp.

3. Hussein Abdel Wahab, Kevin Jeffay: Issues, Problems and Solutions in Sharing X

Clients on Multiple Displays . - Technical Report (TR92-042). UNC-Chapel Hill,

December 1992; ftp://ftp.cs.odu.edu/pub/wahab/XTV/XTV.related.papers/XIssues.ps

4. G. Chung, K. Jeffay, H. Abdel-Wahab, Dynamic Participation in Computer-based

Conferencing System . - Journal of Computer Communications, pp. 7-16, Vol. 17, No. 1,

January 1994; ftp://ftp.cs.odu.edu/pub/wahab/XTV/ XTV.related.papers/ LateJoin.ps

5. Bormann, C, Ou, J, Gehrcke, H-C, Kerschat, T, and Seifert, N, MTP-2: Towards

Achieving the S.E.R.O. Properties for Multicast Transport - In: ICCCN 94, San

Fransico, Sept. 1994, http://www.prz.tu-berlin/~torsten/papers/sero.ps

6. Knight, Jon P.; Multicast Transport Protocols. - High Performance Networks and

Distributed Systems, Archive URL http://hill.lut.ac.uk/DS-Archive/MTP.html

7. S. Armstrong, A. Freier, K. Marzullo Multicast Transport Protocol . IETF RFC 1301,

Feb. 1992.

8. C. Bormann, G. Hoffmann: Xmc and Xy - Scalable Window Sharing and Mobility . - 8th

Annual X Technical Conference, January 1994; http://www.prz.tu-berlin.de/docs/

Publications/TUB-PRZ-W-1187.ps

9. Whetten, B., Kaplan, S. and Montgomery, T., A High Performance Totally Ordered

Multicast Protocol - In: Dagstuhl Distributed Systems Workshop, Sept. 1994,

ftp://research.ivv.nasa.gov/pub/doc/RMP/RMP_dagstuhl.ps

10. Floyd, S., Jacobson, V., Liu, C., McCanne, S., and Zhang, L.: A Reliable Multicast

Framework for Light-weight Sessions and Application Level Framing , in ACM

SIGCOMM 95; file://ftp.ee.lbl.gov/papers/srm.ps.Z

11. Crowcroft, J., Wang, Zh., Smith, A., Adams, J. A Rough Comparison of the IETF and

ATM Service Models . - In IEEE Network, Nov./Dec. 1995 Vol. 9, No 6, pp. 12-16

12. Deering, S., Host Extensions for IP Multicasting , IETF, RFC 1112, Aug., 1989

13. Fenner, W. Internet Group Management Protocol , Version 2, Internet draft, <draft-ietf-

idmr-igmp-v2-01>, September, 1995

14. Laubach, M., Classical IP and ARP over ATM , IETF, RFC 1577, January 1994, 17 p.

15. Baseline Text for MPOA , ATM Forum document [ATMF/95-0824r1]

16. Salgarelli, L., Schulzrinne, H., Roth, R., Smirnov, M. Definition of services provided by

the protocol architecture , MULTICUBE/I/W23/GMD/ 001.02 [I.2301 Release2], 39 pp.

17. Buck, J., Goei, E., Huang, W.-J., Kamas, A., Lee, E. PTOLEMY: Users Manual ,

U.C.Berkeley, Department of EECS, Apr., 1994.

18. ForeRunner ATM Switch User´s Manual . - MANU 0065 - Rev.A - BETA2 - January,

1996, FORE Systems, Inc.,

19. Schulzrinne, H., Guide to isc 1.1 (Integrated Session Controller),

http://www.fokus.gmd.de/step/isc/

20. Smirnov, M. ARP Perfomance Study , - Technical Report, GMD FOKUS, 1996.